Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 17 - LIT-18626-11-70
P. 17

    UF4D13E0.book  Page 12  Wednesday, March 15, 2017  11:08 AM

                                                                         Safety information

                            EJU30831                              EJU30851
                               Recommended equipment                    Hazard information
                            The following items  should be carried on   When transporting  or  storing your water-
                            board your watercraft:                 craft, always turn  the fuel  cock  knob to
                             Sound-signaling device               “OFF”, otherwise gasoline may overflow
                              You should carry a whistle or other sound-  from the carburetor.
                              signaling device that can be used to signal
                              other boats. See “Rules of the Road” for
                              more information.
                             Visual distress signals
                              It is recommended that a U.S. Coast Guard
                              approved pyrotechnic device be stored in a
                              waterproof container on your watercraft. A
                              mirror can also be used as an emergency
                              signal. Contact a  Yamaha  dealer or the
                              U.S. Coast Guard for more information.
                             Watch                                Never start the engine or let it run for any
                              A watch is  helpful so you will know how  length of time in an enclosed area. Exhaust
                              long you have been operating the water-  fumes contain carbon monoxide, a color-
                              craft.                               less, odorless gas that may cause loss of
                             Towline                              consciousness and death within a short
                              A towline can be used to tow a disabled  time. Always operate the watercraft in an
                              watercraft in an emergency.          open area.

                                                                                                   12

| 12 13 14 15 16 17 18 19 20 21 22 |