Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 72 - LIT-18626-11-70
P. 72

    UF4D13E0.book  Page 67  Wednesday, March 15, 2017  11:08 AM

                            Specifications

                            EJU34543                              Drive unit:
                                      Specifications                Propulsion system:
                            Watercraft capacity:                      Jet pump
                              Maximum people on board:              Jet pump type:
                                1 person                              Axial flow, single stage
                            Dimensions and weight:                  Impeller rotation:
                              Length:                                 Counterclockwise
                                2240 mm (88.2 in)                   Jet thrust nozzle angle:
                              Width:                                  P1: 14.4+14.4°
                                680 mm (26.8 in)                      P2: 17.3+17.3°
                              Height:                             Fuel and oil:
                                660 mm (26.0 in)                    Recommended fuel:
                              Dry weight:                             Regular unleaded gasoline
                                139 kg (306 lb)                     Minimum octane rating (PON):
                            Performance:                              86
                              Maximum fuel consumption:             Minimum octane rating (RON):
                                29.0 L/h (7.7 US gal/h, 6.4 Imp.gal/h)  90
                              Cruising range at full throttle:      Recommended engine oil:
                                0.62 hour                             YAMALUBE 2-W or TC-W3 outboard motor
                              Trolling speed:                         oil or equivalent
                                1300 ±50 r/min                      Fuel mixing ratio (fuel to oil):
                            Engine:                                   50 : 1
                              Engine type:                          Fuel tank total capacity:
                                2-stroke                              18 L (4.8 US gal, 4.0 Imp.gal)
                              Number of cylinders:                  Fuel tank reserve capacity:
                                2                                     5.5 L (1.5 US gal, 1.2 Imp.gal)
                              Engine displacement:
                                701 cm³
                              Bore × stroke:
                                81.0 × 68.0 mm (3.19 × 2.68 in)
                              Compression ratio:
                                7.2 : 1
                              Lubrication system:
                                Pre-mixed fuel and oil
                              Cooling system:
                                Water
                              Starting system:
                                Electric
                              Ignition system:
                                C.D.I.
                              Spark plug (NGK):
                                B7HS
                              Spark plug gap:
                                0.6–0.7 mm (0.024–0.028 in)
                              Battery capacity:
                                12 V, 19 Ah
                              Charging system:
                                Flywheel magneto

                            67

| 67 68 69 70 71 72 73 74 75 76 77 |