Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 38 - LIT-18626-11-70
P. 38

    UF4D13E0.book  Page 33  Wednesday, March 15, 2017  11:08 AM

                            Operation and handling requirements

                            EJU40022                              engine, which can  result in severe  dam-
                                Draining the bilge water
                                                                  age. [ECJ00554]
                            ECJ01302
                             NOTICE
                            Do not run the engine at full throttle when
                            bilge water remains in the engine com-
                            partment. The bilge water can splash into
                            the engine, which can result  in  severe
                            damage.
                            EJU40922
                            Draining the bilge water on water
                            A small quantity of bilge water will remain in
                            the engine compartment even after the bilge
                            water is drained on water. To completely re-
                            move the bilge water, remove the watercraft
                            from the  water and wipe up any  remaining
                            moisture in the engine compartment with a
                            dry cloth.
                            Jet vacuum bilge draining system
                            While the watercraft is operating, bilge water
                            in the engine compartment is drawn in by the
                            vacuum that is generated in the jet pump and
                            discharged from the watercraft through the
                            jet thrust nozzle.
                            To drain the bilge water on water:
                            Operate the watercraft as straight as possible
                            and above planing speed for at least 2 minu-
                            tes. NOTICE: Do not run the engine at full
                            throttle for at least 1 minute after the en-
                            gine has been restarted. Bilge water in the
                            engine compartment can splash into the

                            33

| 33 34 35 36 37 38 39 40 41 42 43 |