Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 77 - LIT-18626-11-70
P. 77

    UF4D13E0.book  Page 72  Wednesday, March 15, 2017  11:08 AM

                                                                           Trouble recovery

                            (4) Open  the fuse  holder and replace the   The towline should be long enough so
                                fuse with one of the correct amperage.  that the watercraft will not collide with
                                WARNING! Do not use fuses of a dif-  the towing boat when slowing down.
                                ferent amperage than recommended.
                                                                  If the watercraft becomes inoperative in the
                                Substitution with a fuse that has  an
                                                                  water, it can be towed to shore.
                                improper rating can cause extensive
                                                                  To tow the watercraft:
                                electrical system damage and possi-
                                                                  Use a towline that is three times the com-
                                ble fire. [EWJ00803]
                                                                  bined length of the towing boat and the wa-
                                                                  tercraft.
                                                                  (1) Securely attach the towline to the bow
                                                                     rope hole of the watercraft being towed.

                              1 Fuse holder
                              2 Electrical box
                              3 Fuse                                 1
                              4 Cap
                                                                   1 Bow rope hole
                              Fuse amperage:
                                Battery fuse:                     (2) Ride the watercraft with  your body
                                  10 A                               weight supported on the riding tray. Hold
                                                                     on to the handlebars in order to balance
                            (5) Insert the fuse holder into the electrical  the watercraft and keep the bow up out
                                box.                                 of the water. NOTICE: The bow must be
                            (6) Securely install the cap by tightening it  kept up out of the water during tow-
                                until it stops.                      ing, otherwise water could flood  the
                            (7) Securely install the  hood in its original  engine compartment or water  could
                                position.                            flow back into the engine, causing se-
                            EJU34705                                 vere engine damage. [ECJ01331]
                            Towing the watercraft
                                                                  Tow the watercraft at 8 km/h (5 mph) or less.
                            EWJ00812
                                                                  NOTICE: Tow the watercraft at 8 km/h (5
                                 WARNING
                                                                  mph) or less, otherwise water could flood
                             The  operator of the  towing boat must
                                                                  the engine  compartment or water could
                              keep  speed to a minimum  and avoid
                                                                  flow back into the engine, causing severe
                              traffic or obstacles which could be  a
                                                                  engine damage. [ECJ01322]
                              hazard to  the operator  on the water-
                              craft.

                                                                                                   72

| 72 73 74 75 76 77 78 79 80 81 82 |