Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 78 - LIT-18626-11-70
P. 78

    UF4D13E0.book  Page 73  Wednesday, March 15, 2017  11:08 AM

                            Trouble recovery

                            EJU34735
                            Submerged watercraft
                            If the watercraft is submerged or flooded with
                            water, drain the bilge water from the engine
                            compartment. Then, have a Yamaha dealer
                            service the watercraft as soon as possible.
                            (1) Remove the watercraft from the water,
                                and then remove the hood.
                            (2) Turn the fuel cock knob to “OFF”.
                            (3) Turn the watercraft over far enough to
                                drain the bilge  water from  the  engine
                                compartment.  NOTICE: Turning the
                                watercraft on its side with the hood
                                removed could cause damage to the
                                steering pole. Use two people to pro-
                                vide enough support to make sure
                                that the steering pole is not damaged.
                                [ECJ00702]
                            (4) Turn the watercraft upright again.
                            (5) Have the watercraft serviced  by a
                                Yamaha  dealer as soon  as possible.
                                NOTICE:  Be  sure to have a  Yamaha
                                dealer inspect the watercraft. Other-
                                wise, serious engine damage could
                                result. [ECJ00792]

                            73

| 73 74 75 76 77 78 79 80 81 82 83 |