Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 59 - LIT-18626-11-70
P. 59

    UF4D13E0.book  Page 54  Wednesday, March 15, 2017  11:08 AM

                                                                           Care and storage

                            EJU41192                              See the instructions included with the flush
                                   Post-operation care
                                                                  kit for proper installation.
                            EWJ00321
                                                                  (1) Place the watercraft in a horizontal posi-
                                 WARNING
                                                                     tion.
                            Always turn the fuel cock knob to “OFF”
                                                                  (2) Remove the hood. (See page 27 for hood
                            when  storing the watercraft,  otherwise
                                                                     removal and installation procedures.)
                            fuel could leak out into the engine or en-
                                                                  (3) Insert the garden hose adapter into the
                            gine compartment, which would create a
                                                                     flushing hose connector.
                            fire hazard.

                                                                   1 Garden hose adapter
                                                                   2 Flushing hose connector
                            After using the watercraft, always take it out
                                                                  (4) Connect the garden hose  adapter to a
                            of the water, clean it, and store it. Leaving the
                                                                     garden hose.
                            watercraft in the water for extended periods
                                                                  (5) Connect the garden hose to a water tap.
                            will accelerate the rate of normal deteriora-
                                                                  (6) Make sure that the area around the wa-
                            tion of the jet pump and hull. Marine organ-
                                                                     tercraft is  clear, and then  start the en-
                            isms  and corrosion  are some of the
                                                                     gine. Immediately after the engine starts,
                            conditions that can shorten the life of many
                                                                     turn the water supply on gradually until
                            watercraft components.
                                                                     water flows out  continually from  the
                            EJU3350B
                            Flushing the cooling water passages      cooling water pilot outlet.
                            ECJ01361
                             NOTICE
                            Do not run the engine for more than 15
                            seconds on land without supplying water,
                            otherwise the engine could overheat.
                            Flush the cooling water passages to prevent
                            them from clogging with salt, sand, or dirt.
                            Use the Yamaha Watercraft Flush Kit to make
                            flushing easier. The flush  kit is  an  optional
                            part.  To purchase  the flush kit,  contact a
                            Yamaha dealer.                        (7) Run the engine at idling speed for about
                                                                     3 minutes watching the engine condition.

                                                                                                   54

| 54 55 56 57 58 59 60 61 62 63 64 |