Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 44 - LIT-18626-11-70
P. 44

    UF4D13E0.book  Page 39  Wednesday, March 15, 2017  11:08 AM

                            Pre-operation checks

                            Add fuel if necessary. (See page 32 for infor-  aged, obstructed, or not connected prop-
                            mation on filling the fuel tank.)     erly. [EWJ00452]
                            EJU32424
                            Water separator check
                            Make sure that no water has collected in the
                            water separator. If water has collected in the
                            water separator, drain it. (See page 26 for in-
                            formation on draining the water separator.)

                                       1

                                       2
                                                                   1 Positive (+) battery terminal: Red lead
                                                                   2 Negative (–) battery terminal: Black lead
                                                                   3 Breather hose
                                                                  Make sure  that the electrolyte level is be-
                                                                  tween the minimum and maximum level
                                                                  marks. WARNING! Never operate the wa-
                              1 Water separator
                                                                  tercraft if the battery does not have suffi-
                              2 Drain screw
                                                                  cient  power to  start the engine or if  it
                            EJU40182
                            Engine unit check                     shows any other signs of decreased pow-
                            Check the exterior of the engine unit for dam-  er. Loss of battery power may leave you
                            age or other problem.                 stranded. [EWJ01241]
                            EJU41012
                            Bilge water check
                            Make sure that no bilge water has collected in
                            the engine compartment. If bilge water has
                            collected in the engine compartment, wipe it
                            up with a dry cloth. NOTICE: Excessive wa-
                            ter in the engine compartment can splash
                            into the engine, which can result in severe
                            damage. [ECJ00342]
                            EJU32485
                            Battery checks
                            Make  sure that  the battery terminals and  1 Maximum level mark
                            breather hose are not damaged and that the  2 Minimum level mark
                            battery leads and breather hose are connect-  Make sure that the battery is securely held in
                            ed properly.  WARNING! Fire or explosion  place.
                            could result if the breather hose is dam-  EJU32614
                                                                  Steering system checks
                                                                  Turn the handlebars to the right and left sev-
                                                                  eral times  to  make sure that operation is
                                                                  smooth and unrestricted throughout the

                            39

| 39 40 41 42 43 44 45 46 47 48 49 |