Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 67 - LIT-18626-11-70
P. 67

    UF4D13E0.book  Page 62  Wednesday, March 15, 2017  11:08 AM

                                                                                 Maintenance

                            (3) Remove the steering cable pivot bolt.  TIP:
                                                                  The outermost  hole in the steering column
                                                                  cannot be used.

                              1 Steering cable pivot bolt
                              2 Steering column
                            (4) Select the nozzle angle, install the steer-  1 Nozzle angles
                                ing cable pivot bolt with the lock washer
                                in the desired position (P1 or P2) on the
                                steering column, and  then tighten  the
                                bolt to the specified torque.

                                                                   1 Nozzle angles
                                                                   2 Steering cable pivot bolt positions
                                                                    Standard steering cable pivot bolt posi-
                                                                    tion:
                                                                      P2
                                                                    Tightening torque:
                                                                      Steering cable pivot bolt:
                                                                        5.4 N·m (0.55 kgf·m, 4.0 lb·ft)

                                                                  (5) Securely connect the steering cable joint
                                                                     to the steering cable pivot bolt.
                                                                  (6) Securely install the steering pole cover
                                                                     and two bolts in their original positions.

                                                                                                   62

| 62 63 64 65 66 67 68 69 70 71 72 |