Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 51 - LIT-18626-11-70
P. 51

    UF4D13E0.book  Page 46  Wednesday, March 15, 2017  11:08 AM

                                                                                      Operation

                            (2) Turn the fuel cock knob to “ON”.  (4) Pull the choke knob all the way out to
                                                                     start a cold engine.

                            (3) Attach the engine shut-off cord (lanyard)
                                to your left wrist, and then attach the clip  TIP:
                                to the engine shut-off switch. (See page  The choke should not be used when the en-
                                23 for information on operating the en-  gine is warm.
                                gine shut-off switch.) WARNING! Check  (5) While lightly squeezing the throttle lever,
                                that the engine shut-off cord (lanyard)  push the start switch (green button) to
                                is attached  correctly. If the engine  start the engine. (See page 23 for infor-
                                shut-off cord (lanyard) is not attached  mation on operating the start switch.)
                                correctly, it may not pull free when the  WARNING! Do  not apply  too much
                                operator falls off, allowing the water-  throttle when starting the engine, oth-
                                craft to continue to run and cause an  erwise the watercraft will  accelerate
                                accident. [EWJ00582]                 unexpectedly. This could cause a col-
                                                   1    2            lision or cause the operator to be
                                                                     thrown overboard. [EWJ00592]

                                                                                     START
                                                3

                              1 Clip
                              2 Engine shut-off switch
                              3 Engine shut-off cord (lanyard)
                                                                  (6) After the  engine has  warmed up,  push
                                                                     the choke knob in to its original position.
                                                                  TIP:
                                                                  If the choke knob is left pulled out, the engine
                                                                  will stall.

                                                                                                   46

| 46 47 48 49 50 51 52 53 54 55 56 |