Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 61 - LIT-18626-11-70
P. 61

    UF4D13E0.book  Page 56  Wednesday, March 15, 2017  11:08 AM

                                                                           Care and storage

                            (4) Unhook the battery bands, and then re-  the battery, otherwise battery life could be
                                move the battery from the watercraft.  shortened. [ECJ00242]

                              1 Positive (+) battery terminal: Red lead  1 Maximum level mark
                              2 Battery band                       2 Minimum level mark
                              3 Negative (–) battery terminal: Black lead
                                                                  If distilled water was added, check the bat-
                              4 Breather hose
                                                                  tery voltage.
                            Checking the battery                  It is recommended to have a Yamaha dealer
                             Make sure that the battery case is not dam-  check the battery voltage and charge the bat-
                              aged.                               tery. If you  charge the battery  yourself, be
                             Make  sure that the  battery terminals are  sure to read and follow the instructions pro-
                              not corroded or damaged.            vided with the battery tester and charger you
                             Make sure that the breather  hose  is not  use. NOTICE: Do not attempt to charge a
                              clogged or damaged.                 battery hastily. Battery life could be short-
                            Checking the electrolyte level
                                                                  ened. [ECJ00252]
                            Make sure  that the electrolyte level  is be-
                                                                  Checking the battery bands
                            tween the maximum and minimum level   Make sure  that  the battery bands are  not
                            marks.                                damaged.
                            If the electrolyte level is low, add distilled wa-
                            ter to raise it to the specified level. NOTICE:
                            Use  only distilled water for  replenishing

                                                                   1 Battery band
                                                                  To store the battery:
                                                                  (1) Clean the battery case using fresh water.

                                                                                                   56

| 56 57 58 59 60 61 62 63 64 65 66 |