Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 34 - LIT-18626-11-70
P. 34

    UF4D13E0.book  Page 29  Wednesday, March 15, 2017  11:08 AM

                            Equipment operation

                            (2) Unfasten the  bands,  and then remove  To open the fire extinguisher container:
                                the storage pouch.                (1) Lift the steering pole and support it with
                                                                     the lock pin.

                              1 Storage pouch
                              2 Band                               1 Steering pole
                                                                   2 Lock pin
                            To install the storage pouch:
                            (1) Bend the owner’s/operator’s manual  (2) Grasp the tab, pull the band to the rear,
                                slightly to insert it into the storage pouch,  and then pull it up.
                                and then add the tool kit and any other
                                small items. Fold the pouch, and  then
                                wrap the strap around it.

                                                                   1 Fire extinguisher container
                                                                   2 Tab
                                                                  (3) Lift the fire extinguisher container about
                              1 Strap                                30  degrees  from the storage position.
                            (2) Install the  storage  pouch on the hood  NOTICE: Do not force  the  fire extin-
                                and secure it with the bands.        guisher container up more than 30 de-
                            (3) Securely install the  hood in its original  grees from the storage position,
                                position.                            otherwise the container and hood
                            EJU41004                                 could be damaged. [ECJ00402]
                            Fire extinguisher container
                            The fire extinguisher container is located on
                            the hood.

                            29

| 29 30 31 32 33 34 35 36 37 38 39 |