Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 37 - LIT-18626-11-70
P. 37

    UF4D13E0.book  Page 32  Wednesday, March 15, 2017  11:08 AM

                                             Operation and handling requirements

                            (2) To mix them thoroughly, shake the con-
                                                                    Fuel tank capacity:
                                tainer from side to side.             Total:
                                                                        18 L (4.8 US gal, 4.0 Imp.gal)
                                                                      Reserve:
                                                                        5.5 L (1.5 US gal, 1.2 Imp.gal)

                                                                  (6) Stop filling when the fuel level just reach-
                                                                     es the bottom of the filler tube. Do not fill
                                                                     up the filler tube. Because fuel expands
                                                                     when it heats up, heat from the engine or
                                                                     the sun can cause fuel to spill out of the
                                                                     fuel  tank. Do not leave the watercraft
                                                                     with a full tank in direct sunlight.
                              1 2-stroke engine oil
                              2 Gasoline                          (7) Wipe up any spilled fuel immediately with
                                                                     a dry cloth.
                            EJU41492
                            Filling the fuel tank                 (8) Securely install the fuel filler cap by tight-
                            To fill the fuel tank:                   ening it until it clicks.
                            (1) Before refueling, stop the engine. Do not  (9) Securely install the hood in its original
                                stand or sit on the watercraft. Never refu-  position.
                                el while smoking, or while in the vicinity
                                of sparks, open flames, or other sources
                                of ignition.
                            (2) Place the watercraft in a well-ventilated
                                area and in a horizontal position.
                            (3) Remove the hood, and then check the
                                fuel level. (See page 27 for hood removal
                                and installation procedures.)
                            (4) Loosen the fuel filler cap and remove it.

                                                    1
                              1 Fuel filler cap
                            (5) Slowly add fuel to the fuel tank.

                                                                                                   32

| 32 33 34 35 36 37 38 39 40 41 42 |