Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 63 - LIT-18626-11-70
P. 63

    UF4D13E0.book  Page 58  Wednesday, March 15, 2017  11:08 AM

                                                                           Care and storage

                            (2) Clean the watercraft. (See page 55 for in-   Throttle cable (throttle lever end)
                                formation on cleaning the watercraft.)  Squeeze the throttle lever and remove the
                                Wax the  hull with a non-abrasive wax  seal. Spray Yamaha Lube-Zall into the out-
                                such as Yamalube Professional Polish.  er cable. Refit the seal securely.
                            EJU40785
                            Lubrication
                            Use a Yamaha Power Cable Luber and spray
                            Yamaha Lube-Zall between the inner and
                            outer cables to lubricate  the cables  and
                            purge out any dirt and moisture.
                            To  keep  moving parts sliding or rotating
                            smoothly, lubricate them with water-resistant
                            grease.
                              Recommended water-resistant grease:
                                YAMALUBE MARINE GREASE             1 Seal
                                                                   Steering cable ball joint (handlebar end)
                             Throttle cable (carburetor end) and choke  and steering cable  inner  wire (handlebar
                              cable (carburetor end)               end)
                                                                   To access the steering cable ball joint (han-
                                                                   dlebar end) and steering cable inner wire
                                                                   (handlebar end), remove the steering pole
                                                                   cover. (See step 1 in “Adjusting the jet
                                                                   thrust nozzle angle” on page 61 for infor-
                                                                   mation on removing the steering pole cov-
                                                                   er.)

                                                                                                   58

| 58 59 60 61 62 63 64 65 66 67 68 |