Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 107 - LIT-18626-11-71
P. 107

    UF4E12E0.book  Page 102  Thursday, June 15, 2017  1:12 PM

                                                                           Trouble recovery

                                use fuses of a different amperage than   The towline should be long enough so
                                recommended. Substitution with a   that the watercraft will not collide with
                                fuse that has an improper rating can  the towing boat when slowing down.
                                cause extensive electrical  system
                                                                  If the watercraft becomes inoperative in the
                                damage and possible fire. [EWJ00803]
                                                                  water, it can be towed to shore.
                              Fuse amperage:                      To tow the watercraft:
                                Electronic throttle valve fuse:   Use a towline that is three times the com-
                                  10 A                            bined length of the towing boat and the wa-
                                Fuel pump fuse:
                                  10 A                            tercraft.
                                Main relay drive fuse:            (1) Securely attach the towline to the bow
                                  10 A                               eye of the watercraft being towed.
                                Main fuse:
                                  20 A
                                Battery fuse:
                                  30 A
                                SCU fuse:
                                  50 A
                                Security system fuse:
                                  3 A

                            (7) Securely install the fuse box cover in its  1
                                original position.
                            (8) Securely install the electrical box cover in  1 Bow eye
                                its original position.
                                                                  (2) Sit astride the seat and hold on to the
                            (9) Slide the locks to their original positions
                                                                     handlebars in order to balance the water-
                                to securely lock the electrical box cover
                                                                     craft. NOTICE: The bow must be kept
                                in place.
                                                                     up out of the water during towing, oth-
                            (10) Securely install the removable watertight
                                                                     erwise water could  flood the  engine
                                storage compartment and seats in their
                                                                     compartment or  water could flow
                                original positions.
                                                                     back into the engine, causing severe
                            If the fuse immediately blows again, the elec-
                                                                     engine damage. [ECJ01331]
                            trical system may be defective. If this occurs,
                                                                  Tow the watercraft at 8 km/h (5 mph) or less.
                            have a Yamaha dealer service the watercraft.
                                                                  NOTICE: Tow the watercraft at 8 km/h (5
                            EJU34716
                            Towing the watercraft                 mph) or less, otherwise water could flood
                            EWJ00812                              the engine  compartment or water could
                                 WARNING                          flow back into the engine, causing severe
                             The  operator of the  towing boat must  engine damage. [ECJ01322]
                              keep  speed to a minimum  and avoid  EJU36156
                              traffic or obstacles which could be  a  Submerged watercraft
                                                                  If the watercraft is submerged or flooded with
                              hazard to  the operator  on the water-
                                                                  water, drain the bilge water from the engine
                              craft.
                                                                                                 102

| 102 103 104 105 106 107 108 109 110 111 112 |