Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 83 - LIT-18626-11-71
P. 83

    UF4E12E0.book  Page 78  Thursday, June 15, 2017  1:12 PM

                                                                                      Operation

                            current location. (See page 36 for shift sys-  bles or sand could be sucked into the jet
                            tem operation procedures.)            intake, causing impeller damage and en-
                                                                  gine overheating. [ECJ00473]

                                                                               60 cm (2 ft)

                                             1
                              1 “N” (Neutral position)
                                                                  TIP:
                                                                  This watercraft is equipped with a reboarding
                                                                  step, which can be lowered and used to as-
                                                                  sist in reboarding. (See page 49 for informa-
                                                                  tion on operating the reboarding step.)
                                                                  EJU36354
                                                                  Boarding alone
                                                                  (1) From the rear of  the  watercraft,  place
                                                                     both hands on the boarding platform,
                                                                     pull yourself up, and then  grasp the
                                                                     handgrip with one hand.
                            EJU36087
                            Boarding the watercraft
                            EWJ01112
                                 WARNING
                            Be sure the operator and any passengers
                            have practiced  boarding from the water
                            while still close to shore before riding. A
                            person who has made many unsuccessful
                            attempts to get back on  the watercraft
                            may become fatigued and suffer from ex-
                            posure, increasing the risk of injury and
                            drowning.
                            Board the watercraft  in water free from
                            weeds and debris and at least 60 cm (2 ft)
                            deep  from the  bottom of the watercraft.
                            NOTICE: Never run the engine in water
                            that is less than 60 cm (2 ft) deep from the
                            bottom of the watercraft, otherwise peb-

                                                                                                   78

| 78 79 80 81 82 83 84 85 86 87 88 |