Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 48 - LIT-18626-11-71
P. 48

    UF4E12E0.book  Page 43  Thursday, June 15, 2017  1:12 PM

                            Instrument operation

                            EJU43760                              their state before the center turned off, and
                                Multifunction information
                                                                  then the center starts to operate normally.
                                          center                  EJU35027
                                                                  Information display
                            The multifunction information center displays
                                                                  The information display shows watercraft op-
                            various watercraft information.
                                                                  erating conditions.
                                      1      2      3
                                                                               1     2

                                             4
                              1 “UNLOCK” indicator light                    3 4 5 6  7  8
                                                                   1 Tachometer
                              2 Information display
                                                                   2 Speedometer
                              3 “L-MODE” indicator light
                                                                   3 Oil pressure warning indicator
                              4 “WARNING” indicator light
                                                                   4 Engine overheat warning indicator
                            Multifunction information center initial op-
                                                                   5 Check engine warning indicator
                            eration
                                                                   6 Shift indicator
                            When the multifunction information center is
                                                                   7 Fuel level warning indicator
                            activated, all of the display segments come  8 Fuel level meter
                            on. After 2 seconds, the warning indicators in
                                                                  EJU43832
                            the information display go off, and then the  Speedometer
                            center starts to operate normally.    The speedometer shows the watercraft
                            If only the multifunction information center is  speed against water.
                            activated, the “WARNING” indicator light
                            blinks once.
                            TIP:
                            The “UNLOCK” indicator light also comes on
                            as part of the initial operation.
                            The  “UNLOCK” indicator light will go off
                            when the engine is started.
                            Multifunction information center standby
                            state
                            If the  multifunction information center  does           1
                                                                   1 Speedometer
                            not receive any operation input within 25 sec-
                            onds after the engine stops, the center will  By switching the display units, the speed can
                            turn off and enter a standby state. When the  be shown in kilometers per hour “km/h” or
                            engine is started again, the displays return to  miles per hour “MPH”.

                            43

| 43 44 45 46 47 48 49 50 51 52 53 |