Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 49 - LIT-18626-11-71
P. 49

    UF4E12E0.book  Page 44  Thursday, June 15, 2017  1:12 PM

                                                                     Instrument operation

                            TIP:                                  The outer numbers × 1000 r/min and display
                            “MPH” is selected as the display unit at the  segments on the meter show the engine
                            Yamaha factory.                       speed.
                            To switch the speedometer display units:
                            Start the engine, stop the engine, and then
                            push the engine stop switch 3 times, pushing
                            the switch for 0.4 seconds or more each time,
                            before the  multifunction information center
                            turns  off. The speedometer display  units
                            change.
                            To  switch the speedometer display units
                            again, repeat this procedure.
                                                                          1
                                                                   1 Tachometer
                                                                  EJU43891
                                                                  Shift indicator
                                                                  This indicator shows the  reverse  gate shift
                                                                  positions: “F” (forward), “N” (neutral), and “R”
                                                                  (reverse).  (See page 36 for shifting proce-
                                                                  dures.)
                                                 1

                              1 Engine stop switch

                                                                                                  2

                                                                                                  3

                                                                                                  4
                                                                                   1
                                                                   1 Shift indicator
                                                                   2 “F” (Forward position)
                                                                   3 “N” (Neutral position)
                                               1                   4 “R” (Reverse position)
                              1 Speedometer                       EJU31515
                                                                  Fuel level meter
                            EJU31464
                            Tachometer                            The fuel level meter shows the amount of fuel
                            The tachometer shows the engine speed.  remaining in the fuel tank. The amount of re-
                                                                  maining fuel  is  shown using eight display
                                                                  segments, which disappear two at a time as
                                                                  the fuel level decreases.

                                                                                                   44

| 44 45 46 47 48 49 50 51 52 53 54 |