Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 89 - LIT-18626-11-71
P. 89

    UF4E12E0.book  Page 84  Thursday, June 15, 2017  1:12 PM

                                                                           Care and storage

                            EJU37146                              (3) Connect the garden hose  adapter to a
                                   Post-operation care
                                                                     garden hose.
                            EWJ00331
                                 WARNING
                            Always place the watercraft upright in a      1               2
                            horizontal position when storing it, other-
                            wise fuel could leak out into the engine or
                            engine compartment, which could create
                            a fire hazard.
                            After using the watercraft, always take it out
                            of the water, clean it, and store it. Leaving the
                            watercraft in the water for extended periods
                                                                   1 Garden hose adapter
                            will accelerate the rate of normal deteriora-
                                                                   2 Garden hose
                            tion of the jet pump and hull. Marine organ-
                            isms  and corrosion  are some of the  (4) Loosen the flushing hose connector cap
                            conditions that can shorten the life of many  and  remove  it. Insert the garden  hose
                            watercraft components.                   adapter into the flushing hose connector
                            EJU43652                                 by pushing and twisting it until it is se-
                            Flushing the cooling water passages      curely connected.
                            ECJ01311
                             NOTICE
                                                                                           1
                            Do not run the engine over 4000 r/min on
                            land. Also, do not run the engine for more
                                                                                          3
                            than 15 seconds without supplying water,
                            otherwise the engine could overheat.
                                                                             2
                            Flush the cooling water passages to prevent
                            them from clogging with salt, sand, or dirt.
                            (1) Place the watercraft in a horizontal posi-
                                tion.
                                                                   1 Garden hose adapter
                            (2) Remove the seats and removable water-
                                                                   2 Flushing hose connector
                                tight storage compartment. (See page 48
                                                                   3 Flushing hose connector cap
                                for seat removal and installation proce-
                                                                  (5) Connect the garden hose to a water tap.
                                dures and page 53 for information on the
                                                                  (6) Make sure that the area around the wa-
                                removable watertight storage compart-
                                                                     tercraft is  clear, and then  start the en-
                                ment.)
                                                                     gine. Immediately after the engine starts,
                                                                     fully turn the water supply on so that wa-

                                                                                                   84

| 84 85 86 87 88 89 90 91 92 93 94 |