Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 75 - LIT-18626-11-71
P. 75

    UF4E12E0.book  Page 70  Thursday, June 15, 2017  1:12 PM

                                                                    Pre-operation checks

                            Securely install the stern drain plugs by tight-  EJU40553
                                                                  Cooling water pilot outlet check
                            ening them until they stop.
                                                                  Make sure that water is discharged from the
                                                                  cooling water pilot outlet while the engine is
                                                                  running. (See page 34 for information on the
                                                                  cooling water pilot outlet.)

                                           1

                              1 Stern drain plug
                            EJU43810
                            Hood check
                            Push down the hood latch and make sure
                            that it is securely closed.           EJU32715
                                                                  Multifunction information center check
                                                                  Make sure that the multifunction information
                                                                  center operates properly. (See page 43 for in-
                                                                  formation on proper operation of the multi-
                                                                  function information center.)

                            EJU40146
                            Post-launch checks
                            Perform the post-launch checks in the pre-
                            operation checklist while the watercraft is in
                            the water and the engine is running.
                            To perform the post-launch checks:    EJU43392
                                                                  Shift system check
                            (1) Launch the watercraft. (See page 73 for
                                                                  Operate the throttle lever and RiDE lever, and
                                information on launching the watercraft.)
                                                                  check that the watercraft moves or does not
                            (2) Perform the checks and make sure that
                                                                  move according to the displayed shift indica-
                                there are no malfunctioning items or oth-
                                                                  tor. (See page 36 for shift system operation
                                er problems.
                                                                  procedures.)  WARNING! To avoid colli-
                                                                  sions, operate at safe speeds and keep a

                                                                                                   70

| 70 71 72 73 74 75 76 77 78 79 80 |