Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 93 - LIT-18626-11-71
P. 93

    UF4E12E0.book  Page 88  Thursday, June 15, 2017  1:12 PM

                                                                           Care and storage

                            EJU33493                               Steering cable (jet thrust nozzle end)
                                   Long-term storage
                            EWJ00331
                                 WARNING
                            Always place the watercraft upright in a
                            horizontal position when storing it, other-
                            wise fuel could leak out into the engine or
                            engine compartment, which could create
                            a fire hazard.
                            Storage for long periods of time, such as win-
                            ter storage, requires preventive maintenance
                            to ensure against deterioration. It is advisable   Shift rod (reverse gate end) and ball joint
                            to have the watercraft serviced by a Yamaha
                            dealer prior to storage.
                            However,  the following  procedures can be
                            performed easily by the owner.
                            EJU40256
                            Cleaning
                            (1) Flush the cooling water passages. (See
                                page 84 for information on flushing the
                                cooling water passages.)
                            TIP:
                            If you will be storing the watercraft for a pro-
                                                                  TIP:
                            longed period, such as winter storage, top off
                                                                  Disconnect the shift rod from the ball joint be-
                            the fuel tank with fresh gasoline and add one
                                                                  fore lubricating.
                            ounce of Yamalube Fuel Stabilizer & Condi-
                                                                  EJU40263
                            tioner Plus to each gallon of fuel in the fuel  Rustproofing
                            tank before starting the engine.      Spray metallic parts of the hull, deck, and en-
                            (2) Clean the watercraft. (See page 85 for in-  gine with a rust inhibitor such as Yamalube
                                formation on cleaning the watercraft.)  Silicone Protectant & Lubricant.
                                Wax the  hull with a non-abrasive wax  Have a Yamaha dealer rustproof the internal
                                such as Yamalube Professional Polish.  engine components.
                            EJU43671
                            Lubrication
                            To  keep  moving parts sliding or rotating
                            smoothly, lubricate them with water-resistant
                            grease.
                              Recommended water-resistant grease:
                                YAMALUBE MARINE GREASE

                                                                                                   88

| 88 89 90 91 92 93 94 95 96 97 98 |