Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 99 - LIT-18626-11-71
P. 99

    UF4E12E0.book  Page 94  Thursday, June 15, 2017  1:12 PM

                                                                                Specifications

                            EJU34543                                Spark plug gap:
                                      Specifications                  0.8–0.9 mm (0.031–0.035 in)
                            Watercraft capacity:                    Battery capacity:
                              Maximum people on board:                12 V, 19 Ah
                                3 person                            Charging system:
                              Maximum load capacity:                  Flywheel magneto
                                240 kg (530 lb)                   Drive unit:
                            Dimensions and weight:                  Propulsion system:
                              Length:                                 Jet pump
                                3350 mm (131.9 in)                  Jet pump type:
                              Width:                                  Axial flow, single stage
                                1220 mm (48.0 in)                   Impeller rotation:
                              Height:                                 Counterclockwise
                                1190 mm (46.9 in)                   Jet thrust nozzle angle:
                              Dry weight:                             24+24 °
                                348 kg (767 lb)                   Fuel and oil:
                            Performance:                            Recommended fuel:
                              Maximum fuel consumption:               Regular unleaded gasoline
                                48.5 L/h (12.8 US gal/h, 10.7 Imp.gal/h)  Minimum octane rating (PON):
                              Cruising range at full throttle:        86
                                1.44 hour                           Minimum octane rating (RON):
                              Trolling speed:                         90
                                1300 ±100 r/min                     Recommended engine oil:
                            Engine:                                   YAMALUBE 4W or 4-stroke motor oil
                              Engine type:                          Recommended engine oil type SAE:
                                Liquid cooled 4-stroke, DOHC          SAE 10W-30, 10W-40, 20W-40, 20W-50
                              Number of cylinders:                  Recommended engine oil grade API:
                                4                                     API SG, SH, SJ, SL
                              Engine displacement:                  Fuel tank total capacity:
                                1812 cm³                              70 L (18.5 US gal, 15.4 Imp.gal)
                              Bore × stroke:                        Engine oil quantity with oil filter replacement:
                                86.0 × 78.0 mm (3.39 × 3.07 in)       3.6 L (3.81 US qt, 3.17 Imp.qt)
                              Compression ratio:                    Engine oil quantity without oil filter replacement:
                                11.0 : 1                              3.5 L (3.70 US qt, 3.08 Imp.qt)
                              Valve clearance-intake (cold):        Engine oil total quantity:
                                0.14–0.23 mm (0.0055–0.0091 in)       5.3 L (5.60 US qt, 4.66 Imp.qt)
                              Valve clearance-exhaust (cold):
                                0.28–0.37 mm (0.0110–0.0146 in)
                              Lubrication system:
                                Wet sump
                              Cooling system:
                                Water
                              Starting system:
                                Electric
                              Ignition system:
                                T.C.I.
                              Spark plug (NGK):
                                LFR6A

                                                                                                   94

| 94 95 96 97 98 99 100 101 102 103 104 |