Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 73 - LIT-18626-11-71
P. 73

    UF4E12E0.book  Page 68  Thursday, June 15, 2017  1:12 PM

                                                                    Pre-operation checks

                            yard) may not pull free when the operator  To check the operation of the switches:
                            falls off, allowing the watercraft to conti-  (1) If the lock mode is selected for the
                            nue to run and cause an accident. [EWJ01221]  Yamaha Security System setting, select
                                                                     the unlock mode. (See  page 31 for
                                                                     Yamaha Security System setting proce-
                                                                     dures.)
                                                                  (2) Push the start switch to make sure that
                                                                     the engine starts.
                                                                  (3) As  soon as the  engine starts running,
                                                                     push the engine stop switch to  make
                                                                     sure that the engine stops immediately.
                                                                  (4) Restart the engine, and then pull the en-
                                                                     gine  shut-off cord (lanyard) to  remove
                            EJU32676                                 the clip from the engine shut-off switch
                            Switch checks
                                                                     to make sure that the engine stops im-
                            ECJ01311
                             NOTICE                                  mediately.
                                                                  EJU40102
                            Do not run the engine over 4000 r/min on  Storage compartment checks
                            land. Also, do not run the engine for more  Make sure  that the storage  compartments
                            than 15 seconds without supplying water,  are not damaged and that water has not col-
                            otherwise the engine could overheat.  lected in the compartments. (See page 51 for
                                                                  information on the storage compartments.)
                            Check the start switch, the engine stop  EJU43800
                            switch, and  the engine shut-off  switch for  Fire extinguisher holder, cover, and band
                            proper operation. (See pages 32 to 32 for in-  checks
                                                                  Make sure that the fire extinguisher holder,
                            formation on operating each switch.)
                                                                  cover, and band are not damaged and that
                                               1                  the fire extinguisher is securely held in place
                                                                  using the band. (See page 53 for information
                                                        3         on the fire extinguisher holder, cover, and
                                                                  band.)

                                                         4

                                           2         5

                              1 Start switch
                              2 Engine stop switch
                              3 Engine shut-off switch
                              4 Clip
                              5 Engine shut-off cord (lanyard)

                                                                                                   68

| 68 69 70 71 72 73 74 75 76 77 78 |