Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 66 - LIT-18626-11-72
P. 66

    UF2T17E0.book  Page 61  Thursday, June 22, 2017  3:15 PM

                            Equipment operation

                            EJU42391                                 hood is securely closed before using the
                            Fire extinguisher holder and cover
                                                                     watercraft.
                            The fire extinguisher holder and cover are lo-
                            cated in the bow storage compartment.
                            To use the fire extinguisher holder and cover:
                            (1) Pull the hood latch rearward, and then lift
                                up the rear of the hood.

                                                         1

                              1 Hood latch
                            (2) Unhook the band and remove the fire ex-
                                tinguisher cover.

                                        1
                                            2

                              1 Fire extinguisher holder and cover
                              2 Band
                            (3) Place the fire extinguisher in the holder,
                                and then place the cover over the fire ex-
                                tinguisher.
                            (4) Securely fasten the cover and the fire ex-
                                tinguisher with the band.
                            (5) Push the rear of the hood down to se-
                                curely lock it in place. Make sure that the

                            61

| 61 62 63 64 65 66 67 68 69 70 71 |