Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 83 - LIT-18626-11-72
P. 83

    UF2T17E0.book  Page 78  Thursday, June 22, 2017  3:15 PM

                                                                    Pre-operation checks

                            EJU32715                              safe distance away from people, objects,
                            Multifunction information center check
                            Make sure that the multifunction information  and other watercraft. [EWJ01860]
                            center operates properly. (See page 44 for in-  1
                            formation on proper operation of the multi-                          2
                            function information center.)

                                                                                                 3

                                                                                                 4

                                                                   1 Shift indicator
                                                                   2 “F” (Forward position)
                                                                   3 “N” (Neutral position)
                                                                   4 “R” (Reverse position)
                                                                  EJU43400
                                                                  Trim indicator check
                                                                  Operate the electric trim switches and check
                                                                  that the trim indicator shows the correct trim
                                                                  angle of the jet thrust nozzle. (See page 38 for
                                                                  electric trim system operation procedures.)

                            EJU43392                                                              1
                            Shift system check
                            Operate the throttle lever and RiDE lever, and
                            check that the watercraft moves or does not
                            move according to the displayed shift indica-
                            tor. (See page 36 for shift system operation
                            procedures.)  WARNING! To avoid colli-  1 Trim indicator
                            sions, operate at safe speeds and keep a  EJU40172
                                                                  Engine idling speed check
                                                                  Start the engine and warm it up. Use the ta-
                                                                  chometer in the multifunction  information
                                                                  center to make sure  that the engine  idling
                                                                  speed is not significantly above or below the
                                                                  specified range.
                                                                    Engine idling speed:
                                                                      1300 ±100 r/min

                                                                                                   78

| 78 79 80 81 82 83 84 85 86 87 88 |