Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 54 - LIT-18626-11-72
P. 54

    UF2T17E0.book  Page 49  Thursday, June 22, 2017  3:15 PM

                            Instrument operation

                            ously. At the same time, the engine speed is  EJU42281
                                                                  Check engine warning
                            limited.
                                                                  If a sensor malfunction or a short circuit is de-
                                                                  tected,  the check engine  warning indicator
                                                                  and the “WARNING” indicator light blink, and
                                                                  the buzzer sounds intermittently.

                            If the engine overheat warning is activated,
                            immediately reduce the engine speed, return
                            to shore, and then make sure that water is
                            being discharged from the cooling water pilot
                                                                  If the check engine warning is activated, im-
                            outlet while the engine is running. If there is
                                                                  mediately reduce the engine speed, return to
                            no discharge of water, stop the engine, and
                                                                  shore, and have a Yamaha dealer check the
                            then check the jet intake for clogging. (See
                                                                  engine.
                            page 105 for information on the jet intake.)
                                                                  TIP:
                            NOTICE: If you cannot locate and correct
                            the  cause of the  overheating, consult  a  Push any  of the  operation buttons  for the
                            Yamaha dealer. Continuing to operate at  multifunction information center to stop the
                            higher speeds could result in severe en-  buzzer.
                                                                  EJU43170
                            gine damage. [ECJ00042]               Multifunction display
                                                                  The multifunction display shows various wa-
                                                                  tercraft and environmental information, such

                            TIP:
                            Push  any of the operation buttons for the
                            multifunction information center to stop the
                            buzzer.

                            49

| 49 50 51 52 53 54 55 56 57 58 59 |