Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 79 - LIT-18626-11-72
P. 79

    UF2T17E0.book  Page 74  Thursday, June 22, 2017  3:15 PM

                                                                    Pre-operation checks

                            right and left fully turned positions of the jet  EJU40363
                                                                  Adjustable tilt steering system checks
                            thrust nozzle.
                                                                  Operate the adjustable tilt steering system
                                                                  several times to make sure that operation is
                                                                  smooth throughout the whole range. Also,
                                                                  make sure that the handlebars are securely
                                                                  locked in place. (See page 34 for adjustable
                                                                  tilt steering system operation procedures.)

                                                                  EJU43213
                                                                  RiDE lever checks
                                                                  Operate the RiDE lever several times to make
                                                                  sure that operation is smooth throughout the
                                                                  whole range. Also, make sure that the RiDE
                                                                  lever returns automatically to its fully closed
                                                                  position when released.

                              Difference between fully turned posi-
                              tions of jet thrust nozzle (distances A
                              and B):
                                Maximum 5 mm (0.20 in)
                                                                  EJU42181
                                                                  Throttle lever checks
                                                                  Operate the throttle lever several times to
                                                                  make sure that operation is smooth through-
                                                                  out the whole range. Also, make sure that the

                                                                                                   74

| 74 75 76 77 78 79 80 81 82 83 84 |