Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 81 - LIT-18626-11-72
P. 81

    UF2T17E0.book  Page 76  Thursday, June 22, 2017  3:15 PM

                                                                    Pre-operation checks

                                to make sure that the engine stops im-
                                                                    Fire extinguisher:
                                mediately.                            Classification:
                            EJU40102                                    B-1
                            Storage compartment checks                Capacity:
                            Make  sure that  the storage compartments   2 lb or more
                            are not damaged and that water has not col-
                            lected in the compartments. (See page 56 for  EJU40122
                                                                  Safety equipment check
                            information on the storage compartments.)
                                                                  Check that safety equipment meeting the ap-
                            EJU41082
                            Fire extinguisher holder, cover, and band   plicable regulations is on board.
                            checks                                EJU32353
                            Make sure that the fire extinguisher holder,  Hull and deck check
                                                                  Check the hull and deck for damage or other
                            cover, and band are not damaged and that
                                                                  problem.
                            the cover is securely held in place using the
                                                                  EJU32657
                            band. (See page 61 for information on the fire  Jet intake checks
                            extinguisher holder, cover, and band.)  Make sure that the jet intake is not damaged
                            EJU32534                              or clogged with weeds or debris. If the jet in-
                            Fire extinguisher check
                            Check that there is a full fire extinguisher on  take is clogged, clean it. (See page 105 for in-
                                                                  formation on the jet intake.)
                            board.
                                                                  EJU43221
                                                                  Jet thrust nozzle and reverse gate check
                                                                  Check the jet thrust nozzle and reverse gate
                                                                  for damage or other problem.
                                                                  EJU44250
                                                                  Stern drain plug checks
                                                                  Loosen the stern drain plugs and  remove
                                                                  them, and then make sure that the plugs and
                                                                  O-rings on the plugs are not damaged and
                                                                  that there is no foreign material on the
                                                                  threads or O-rings on  the plugs.  NOTICE:
                                                                  Before installing  the stern drain plugs,
                            To check  the  fire extinguisher, see the  in-
                                                                  clean the  drain plug threads and the  O-
                            structions supplied  by the fire extinguisher
                                                                  rings on the plugs to remove any foreign
                            manufacturer. Always keep the fire extin-
                                                                  materials, such as dirt or sand. Otherwise,
                            guisher secured in the holder with its cover in
                                                                  the stern drain plugs could be damaged,
                            place.
                                                                  allowing water to enter the engine com-
                            Always carry a fire extinguisher on board. A
                                                                  partment. Check the O-rings on the stern
                            fire extinguisher is not standard  equipment
                                                                  drain plugs and make sure that the plugs
                            with this watercraft. If you do not have one,
                                                                  are tightened securely before launching
                            contact a Yamaha dealer or a fire extinguish-
                                                                  the  watercraft. Otherwise, water may
                            er dealer to obtain one meeting the proper
                            specifications.

                                                                                                   76

| 76 77 78 79 80 81 82 83 84 85 86 |