Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 114 - LIT-18626-11-72
P. 114

    UF2T17E0.book  Page 109  Thursday, June 22, 2017  3:15 PM

                            Trouble recovery

                                                                  If the watercraft becomes inoperative in the
                              Fuse amperage:
                                Electronic throttle valve fuse:   water, it can be towed to shore.
                                  10 A                            To tow the watercraft:
                                Fuel pump fuse:                   Use a towline that is three times the com-
                                  10 A                            bined length of the towing boat and the wa-
                                Main relay drive fuse:
                                  10 A                            tercraft.
                                Main fuse:                        (1) Securely attach the towline to the bow
                                  20 A                               eye of the watercraft being towed.
                                Battery fuse:
                                  30 A
                                SCU fuse:
                                  50 A
                                Bilge pump fuse:
                                  3 A
                                Security system fuse:
                                  3 A

                            (7) Securely install the fuse box cover in its  1
                                original position.
                            (8) Securely install the electrical box cover in  1 Bow eye
                                its original position.
                                                                  (2) Sit astride the seat and hold on to the
                            (9) Slide the locks to their original positions
                                                                     handlebars in order to balance the water-
                                to securely lock the electrical box cover
                                                                     craft. NOTICE: The bow must be kept
                                in place.
                                                                     up out of the water during towing, oth-
                            (10) Securely install the removable watertight
                                                                     erwise water could  flood the  engine
                                storage compartment and seats in their
                                                                     compartment or  water could flow
                                original positions.
                                                                     back into the engine, causing severe
                            If the fuse immediately blows again, the elec-
                                                                     engine damage. [ECJ01331]
                            trical system may be defective. If this occurs,
                                                                  Tow the watercraft at 8 km/h (5 mph) or less.
                            have a Yamaha dealer service the watercraft.
                                                                  NOTICE: Tow the watercraft at 8 km/h (5
                            EJU34716
                            Towing the watercraft                 mph) or less, otherwise water could flood
                            EWJ00812                              the engine  compartment or water could
                                 WARNING                          flow back into the engine, causing severe
                             The  operator of the  towing boat must  engine damage. [ECJ01322]
                              keep  speed to a minimum  and avoid  EJU36156
                                                                  Submerged watercraft
                              traffic or obstacles which could be  a
                                                                  If the watercraft is submerged or flooded with
                              hazard to  the operator  on the water-
                                                                  water, drain the bilge water from the engine
                              craft.
                                                                  compartment. Then, have a Yamaha dealer
                             The towline should be long enough so
                                                                  service the watercraft as soon as possible.
                              that the watercraft will not collide with
                                                                  If the watercraft was submerged:
                              the towing boat when slowing down.
                                                                  (1) Remove the watercraft from  the water
                                                                     and drain  the water  from the  storage
                            109

| 109 110 111 112 113 114 115 116 117 118 119 |