Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 55 - LIT-18626-11-72
P. 55

    UF2T17E0.book  Page 50  Thursday, June 22, 2017  3:15 PM

                                                                     Instrument operation

                            as the shift position and jet thrust nozzle trim  (reverse).  (See page 36 for shifting proce-
                            angle.                                dures.)
                                      1     2        3                     1
                                                                                                 2

                                                                                                 3

                                                                                                 4

                              1 Shift indicator                    1 Shift indicator
                              2 Watercraft information             2 “F” (Forward position)
                              3 Trim indicator                     3 “N” (Neutral position)
                                                                   4 “R” (Reverse position)
                            The display units of the multifunction display
                            are selected according to the display units of  EJU43190
                                                                  Trim indicator
                            the digital speedometer. (To change the dis-
                                                                  This indicator shows the trim angle of the jet
                            play units, see page 45 for digital speedome-
                                                                  thrust nozzle. One of the two upper display
                            ter display selection procedures.)
                                                                  segments will be shown when the trim angle
                            When “km/h” are selected as the  display
                                                                  is increased, and one of the two lower display
                            units of the digital speedometer, values are
                                                                  segments will be shown when the trim angle
                            shown in kilometers/liters/degrees Celsius.
                                                                  is decreased. When the  neutral position of
                            When “mph” are selected as the display units
                                                                  the jet thrust nozzle is selected, the middle
                            of the digital speedometer, values are shown
                                                                  display segment will be shown. (See page 38
                            in miles/gallons/degrees Fahrenheit.
                                                                  for trim angle selection procedures.)
                            EJU43181
                            Shift indicator
                            This indicator shows the  reverse gate  shift
                            positions: “F” (forward), “N” (neutral), and “R”
                                                                                                  1

                                                                   1 Trim indicator
                                                                  EJU43520
                                                                  Watercraft information
                                                                  The multifunction display shows various wa-
                                                                  tercraft and environmental  information. To
                                                                  switch the display mode, push the “MO-

                                                                                                   50

| 50 51 52 53 54 55 56 57 58 59 60 |