Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 65 - LIT-18626-11-72
P. 65

    UF2T17E0.book  Page 60  Thursday, June 22, 2017  3:15 PM

                                                                     Equipment operation

                            To open the built-in watertight storage com-  To  open the removable  watertight storage
                            partment:                             compartment:
                            Loosen the cap and remove it.         (1) Remove the rear seat. (See page 53 for
                                                                     seat  removal and installation proce-
                                                                     dures.)
                                                                  (2) Loosen the cap and remove it.

                                                1

                              1 Cap
                                                                         1

                                                                   1 Cap

                                      1
                              1 Built-in watertight storage compartment

                              Built-in watertight storage compart-       1
                              ment:
                                Capacity:                          1 Removable watertight storage compart-
                                  2.5 L (0.7 US gal, 0.6 Imp.gal)    ment
                                Load limit:                         Removable watertight storage compart-
                                  1.0 kg (2 lb)
                                                                    ment:
                                                                      Capacity:
                            To close the built-in watertight storage com-  9.0 L (2.4 US gal, 2.0 Imp.gal)
                            partment:                                 Load limit:
                            Securely install the cap by tightening it until it  3.0 kg (7 lb)
                            stops.
                            Removable watertight storage compart-  To close the removable watertight storage
                            ment                                  compartment:
                            The removable watertight storage compart-  (1) Securely install the cap by tightening it
                            ment is located under the rear seat.     until it stops.
                                                                  (2) Securely install the rear seat in its original
                                                                     position.

                                                                                                   60

| 60 61 62 63 64 65 66 67 68 69 70 |