Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 39 - LIT-18626-11-72
P. 39

    UF2T17E0.book  Page 34  Thursday, June 22, 2017  3:15 PM

                                                             Control function operation

                            EJU31262                              in response to handlebar input until you apply
                            Steering system
                                                                  throttle again or you reach trolling speed.
                            By turning the handlebars in the direction you
                                                                  EJU31294
                            wish to travel, the angle of the jet thrust noz-  Adjustable tilt steering system
                            zle is changed, and the direction of the water-  The position of the handlebars can be adjust-
                            craft is changed accordingly.         ed back and forth by operating the tilt lever.
                                                                  To adjust the handlebar position:
                                                1                 (1) Pull the tilt lever up to disengage the han-
                                                                     dlebar lock, and then move the handle-
                                                                     bars back or forth to the desired position.
                                                                     WARNING! Never pull the tilt lever dur-
                                                                     ing operation, otherwise the handle-
                                                                     bars may suddenly  change position,
                                                                     which may lead to an accident. [EWJ00042]

                                                                                               1

                                                        2

                              1 Handlebar
                              2 Jet thrust nozzle                  1 Tilt lever
                            Since the strength of the jet thrust determines
                            the speed and degree of a turn, throttle must
                            always  be  applied when attempting a  turn,
                            except at trolling speed.
                            This model is equipped with the Yamaha En-
                            gine Management  System (YEMS) that  in-
                            cludes an off-throttle steering (OTS) system.
                            It will activate at planing speeds should you
                            attempt to steer the watercraft after releasing
                            the throttle lever. The OTS system assists in
                            turning by continuing to supply some thrust
                            while the watercraft is decelerating, but you
                            can turn  more sharply if you apply throttle
                            while turning the handlebars. The OTS sys-
                            tem does not function below planing speeds
                            or when the engine is off. Once the engine
                            slows down, the watercraft will no longer turn

                                                                                                   34

| 34 35 36 37 38 39 40 41 42 43 44 |