Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 61 - LIT-18626-11-72
P. 61

    UF2T17E0.book  Page 56  Thursday, June 22, 2017  3:15 PM

                                                                     Equipment operation

                            could fall, which could result in severe in-  objects that must be kept dry, put them in a
                            jury. [EWJ01511]                      waterproof bag.
                                                                  Make sure  that the storage  compartments
                                                                  are closed securely before operating the wa-
                                                                  tercraft.
                                                                  EJU42211
                                                                  Bow storage compartment
                                                                  The bow storage compartment is located un-
                                1
                                                                  der the hood.
                                                                  To open the bow storage compartment:
                                                                  Pull the hood latch rearward, and then lift up
                                                                  the rear of the hood.
                              1 Cleat
                            EJU34894
                            Pull-up cleats (FX Cruiser HO)                                     1
                            The pull-up cleats are used to attach a rope
                            to the watercraft when mooring it.
                            To use a pull-up cleat, pull it up. The pull-up
                            cleat returns automatically to its original posi-
                            tion when released. WARNING! Do not use
                            the pull-up cleats to lift the watercraft. The
                            pull-up cleats are not designed to support
                                                                   1 Hood latch
                            the watercraft’s weight. If the pull-up
                            cleats break, the watercraft could fall,
                            which could result in severe injury. [EWJ00822]

                                                          1

                                                                                     1

                                                                   1 Bow storage compartment
                                                                    Bow storage compartment:
                                                                      Capacity:
                              1 Pull-up cleat
                                                                        90.0 L (23.8 US gal, 19.8 Imp.gal)
                            EJU42291                                  Load limit:
                            Storage compartments                        5.0 kg (11 lb)
                            This watercraft is equipped with the following
                            storage compartments.
                            Only the securely closed watertight storage
                            compartments are waterproof. If you carry

                                                                                                   56

| 56 57 58 59 60 61 62 63 64 65 66 |