Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 80 - LIT-18626-11-72
P. 80

    UF2T17E0.book  Page 75  Thursday, June 22, 2017  3:15 PM

                            Pre-operation checks

                            throttle lever returns automatically to its fully  EJU32676
                                                                  Switch checks
                            closed (idle) position when released.  ECJ01311
                                                                  NOTICE
                                                                  Do not run the engine over 4000 r/min on
                                                                  land. Also, do not run the engine for more
                                                                  than 15 seconds without supplying water,
                                                                  otherwise the engine could overheat.
                                                                  Check the start switch, the engine stop
                                                                  switch,  and the engine  shut-off switch  for
                                                                  proper operation. (See pages 32 to 32 for in-
                                                                  formation on operating each switch.)
                            EJU40113
                            Remote control transmitter check                        1   2   3
                            Make sure that the remote control transmitter
                            operates properly. (See page 31 for Yamaha
                            Security System setting procedures and
                            page 40 for Low RPM Mode activation pro-
                            cedures.)
                            EJU32664
                            Engine shut-off cord (lanyard) check
                            Make sure that the engine shut-off cord (lan-       4
                            yard) is not damaged. If the cord is damaged,                5
                            replace it.  WARNING! Never try to repair  1 Clip
                                                                   2 Engine shut-off switch
                            the engine shut-off cord (lanyard) or tie it
                                                                   3 Start switch
                            together. The engine  shut-off cord (lan-
                                                                   4 Engine stop switch
                            yard) may not pull free when the operator
                                                                   5 Engine shut-off cord (lanyard)
                            falls off, allowing the watercraft to conti-
                                                                  To check the operation of the switches:
                            nue to run and cause an accident. [EWJ01221]
                                                                  (1) If the lock mode is selected for the
                                                                     Yamaha Security System setting, select
                                                                     the unlock mode. (See  page 31 for
                                                                     Yamaha Security System setting proce-
                                                                     dures.)
                                                                  (2) Push the start switch to make sure that
                                                                     the engine starts.
                                                                  (3) As  soon as the  engine starts running,
                                                                     push the engine stop switch to  make
                                                                     sure that the engine stops immediately.
                                                                  (4) Restart the engine, and then pull the en-
                                                                     gine  shut-off cord (lanyard) to  remove
                                                                     the clip from the engine shut-off switch

                            75

| 75 76 77 78 79 80 81 82 83 84 85 |