Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 82 - LIT-18626-11-72
P. 82

    UF2T17E0.book  Page 77  Thursday, June 22, 2017  3:15 PM

                            Pre-operation checks

                            flood the engine compartment and cause  EJU40146
                                                                  Post-launch checks
                            the watercraft to submerge. [ECJ00363]
                                                                  Perform the post-launch checks in the pre-
                                                                  operation checklist while the watercraft is in
                                                                  the water and the engine is running.
                                                                  To perform the post-launch checks:
                                                           2      (1) Launch the watercraft. (See page 80 for
                                                           1         information on launching the watercraft.)
                                                                  (2) Perform the checks and make sure that
                                                                     there are no malfunctioning items or oth-
                                                                     er problems.
                                                                  EJU40553
                                                                  Cooling water pilot outlet check
                              1 Stern drain plug                  Make sure that water is discharged from the
                              2 O-ring
                                                                  cooling water pilot outlet while the engine is
                            Securely install the stern drain plugs by tight-  running. (See page 35 for information on the
                            ening them until they stop.           cooling water pilot outlet.)
                                                             1

                              1 Stern drain plug
                            EJU41441
                            Hood check
                            Push down on the rear of the hood and make
                            sure that it is securely closed.

                            77

| 77 78 79 80 81 82 83 84 85 86 87 |