Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 57 - LIT-18626-11-72
P. 57

    UF2T17E0.book  Page 52  Thursday, June 22, 2017  3:15 PM

                                                                     Instrument operation

                            TIP:                                  To start the measurements:
                            The  actual fuel consumption varies greatly  Push the “START/STOP” button for less than
                            depending on the operating conditions. Use  1 second. The beeper sounds once and the
                            this function as a reference only.    measurements start.
                                                                  To stop the measurements:
                                                                  Push the “START/STOP” button for less than
                                                                  1 second while the measurements are being
                                                                  recorded. The beeper sounds once and the
                                                                  measurements stop.
                                                                  To restart the measurements:
                                                                  Push the “START/STOP” button for less than
                                                                  1 second while the measurements are
                                                                  stopped. The beeper sounds once and the
                                                                  measurements restart.
                                                                  To reset the measurements:
                            Average speed/Tripmeter modes
                                                                  Push the “MODE/RESET” button for at least
                            Average speed and distance traveled are re-
                                                                  2 seconds while the  measurements are
                            corded once the “START/STOP” button is
                                                                  stopped. The beeper sounds twice and the
                            pushed to start the measurements, regard-
                                                                  measurements are reset.
                            less of the current display.
                            TIP:
                            The measurements are performed only while
                            the engine is running.
                            The measurements are not saved if the en-
                            gine is stopped. The measurements are reset
                            automatically when the  displays  go off  25
                            seconds after the engine stops.

                                                         1

                                                         2

                              1 “START/STOP” button
                              2 “MODE/RESET” button

                                                                                                   52

| 52 53 54 55 56 57 58 59 60 61 62 |