Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 59 - LIT-18626-11-72
P. 59

    UF2T17E0.book  Page 54  Thursday, June 22, 2017  3:15 PM

                                                                     Equipment operation

                            (3) Pull the seat rearward and remove it.  EJU31364
                                                                  Handgrip
                                                                  The handgrip is used when boarding the wa-
                                                                  tercraft from the water and when the spotter
                                                                  is facing rearward. WARNING! Do not use
                                                                  the handgrip to lift the watercraft.  The
                                                                  handgrip is not  designed to support the
                                                                  watercraft’s weight. If the handgrip
                                                                  breaks, the watercraft could  fall, which
                                                                  could result in severe injury. [EWJ00022]

                            To install the front seat:
                            (1) Insert the projection on the front of the
                                seat into the stay on the deck.
                                                                    1

                                                                   1 Handgrip
                                                                  EJU37382
                                                                  Reboarding grip
                                                                  The reboarding grip is used when boarding
                                                                  the watercraft from the water.
                            (2) Push the rear of the seat down to secure-
                                ly lock it in place.

                                                                      1

                                                                   1 Reboarding grip
                                                                  EJU34865
                                                                  Reboarding step
                            (3) Securely install the rear seat in its original  The reboarding step is used to assist in re-
                                position.                         boarding the watercraft from the water.
                                                                  When boarding the watercraft, push the re-
                                                                  boarding step down until it stops. The step
                                                                  returns automatically to its original position

                                                                                                   54

| 54 55 56 57 58 59 60 61 62 63 64 |