Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 106 - LIT-18626-11-72
P. 106

    UF2T17E0.book  Page 101  Thursday, June 22, 2017  3:15 PM

                            Specifications

                            EJU34543                                Spark plug gap:
                                      Specifications                  0.8–0.9 mm (0.031–0.035 in)
                            Watercraft capacity:                    Battery capacity:
                              Maximum people on board:                12 V, 19 Ah
                                3 person                            Charging system:
                              Maximum load capacity:                  Flywheel magneto
                                240 kg (530 lb)                   Drive unit:
                            Dimensions and weight:                  Propulsion system:
                              Length:                                 Jet pump
                                3560 mm (140.2 in)                  Jet pump type:
                              Width:                                  Axial flow, single stage
                                1230 mm (48.4 in)                   Impeller rotation:
                              Height:                                 Counterclockwise
                                1230 mm (48.4 in)                   Jet thrust nozzle angle:
                              Dry weight:                             24+24 °
                                376 kg (829 lb) (FX HO)             Jet thrust nozzle trim angle:
                                377 kg (831 lb) (FX Cruiser HO)       -6, -3, 0, 3, 6 °
                            Performance:                          Fuel and oil:
                              Maximum fuel consumption:             Recommended fuel:
                                48.5 L/h (12.8 US gal/h, 10.7 Imp.gal/h)  Regular unleaded gasoline
                              Cruising range at full throttle:      Minimum octane rating (PON):
                                1.44 hour                             86
                              Trolling speed:                       Minimum octane rating (RON):
                                1300 ±100 r/min                       90
                            Engine:                                 Recommended engine oil:
                              Engine type:                            YAMALUBE 4W or 4-stroke motor oil
                                Liquid cooled 4-stroke, DOHC        Recommended engine oil type SAE:
                              Number of cylinders:                    SAE 10W-30, 10W-40, 20W-40, 20W-50
                                4                                   Recommended engine oil grade API:
                              Engine displacement:                    API SG, SH, SJ, SL
                                1812 cm³                            Fuel tank total capacity:
                              Bore × stroke:                          70 L (18.5 US gal, 15.4 Imp.gal)
                                86.0 × 78.0 mm (3.39 × 3.07 in)     Engine oil quantity with oil filter replacement:
                              Compression ratio:                      3.6 L (3.81 US qt, 3.17 Imp.qt)
                                11.0 : 1                            Engine oil quantity without oil filter replacement:
                              Valve clearance-intake (cold):          3.5 L (3.70 US qt, 3.08 Imp.qt)
                                0.14–0.23 mm (0.0055–0.0091 in)     Engine oil total quantity:
                              Valve clearance-exhaust (cold):         5.3 L (5.60 US qt, 4.66 Imp.qt)
                                0.28–0.37 mm (0.0110–0.0146 in)
                              Lubrication system:
                                Wet sump
                              Cooling system:
                                Water
                              Starting system:
                                Electric
                              Ignition system:
                                T.C.I.
                              Spark plug (NGK):
                                LFR6A

                            101

| 101 102 103 104 105 106 107 108 109 110 111 |