Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 54 - LIT-18626-11-73
P. 54

    UF3J14E0.book  Page 49  Friday, June 23, 2017  9:47 AM

                            Instrument operation

                            ously. At the same time, the engine speed is  EJU42281
                                                                  Check engine warning
                            limited.
                                                                  If a sensor malfunction or a short circuit is de-
                                                                  tected,  the check engine  warning indicator
                                                                  and the “WARNING” indicator light blink, and
                                                                  the buzzer sounds intermittently.

                            If the engine overheat warning is activated,
                            immediately reduce the engine speed, return
                            to shore, and then make sure that water is
                            being discharged from the port (left) cooling
                                                                  If the check engine warning is activated, im-
                            water pilot outlet while the engine is running.
                                                                  mediately reduce the engine speed, return to
                            If there is no discharge of water, stop the en-
                                                                  shore, and have a Yamaha dealer check the
                            gine, and then check the jet intake for clog-
                                                                  engine.
                            ging. (See page 107 for information on the jet
                                                                  TIP:
                            intake.) NOTICE: If you cannot locate and
                            correct the cause of the overheating, con-  Push any  of the  operation buttons  for the
                            sult a Yamaha dealer. Continuing to oper-  multifunction information center to stop the
                            ate at higher speeds could result in severe  buzzer.
                                                                  EJU43170
                            engine damage. [ECJ00042]             Multifunction display
                                                                  The multifunction display shows various wa-
                                                                  tercraft and environmental information, such

                            TIP:
                            Push  any of the operation buttons for the
                            multifunction information center to stop the
                            buzzer.

                            49

| 49 50 51 52 53 54 55 56 57 58 59 |