Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 75 - LIT-18626-11-73
P. 75

    UF3J14E0.book  Page 70  Friday, June 23, 2017  9:47 AM

                                                                       First-time operation

                            EJU42690
                                     Engine break-in
                            ECJ00432
                             NOTICE
                            Failure to perform the engine break-in
                            could result in reduced engine life or even
                            severe engine damage.
                            The engine break-in is essential to allow the
                            various components of the engine to  wear
                            and polish themselves to the correct operat-
                            ing clearances. This ensures proper perfor-
                            mance and promotes longer component life.
                            To perform the engine break-in:
                            (1) Check the engine oil level. (See page 66
                                for information on checking  the  engine
                                oil level.)
                            (2) Launch the watercraft and start the en-
                                gine. (See page 82 for information  on
                                starting the engine.)
                            (3) For the first 5 minutes, operate with the
                                engine speed at 2000 r/min.
                            (4) For the next 90 minutes, operate with the
                                engine speed below 5000 r/min.
                            After the engine break-in is complete, the wa-
                            tercraft can be operated normally.

                                                                                                   70

| 70 71 72 73 74 75 76 77 78 79 80 |