Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 70 - LIT-18626-11-73
P. 70

    UF3J14E0.book  Page 65  Friday, June 23, 2017  9:47 AM

                            Operation and handling requirements

                            (4) Pull the hood latch rearward, and then lift  of the fuel tank. Do not overfill the fuel
                                up the rear of the hood.             tank. Because fuel expands when it
                                                                     heats up, heat from the engine or the sun
                                       1                             can cause fuel to spill out of the fuel tank.
                                                                     Do not  leave the watercraft with  a full
                                                                     tank in direct sunlight.

                              1 Hood latch                                                1
                            (5) Loosen the fuel filler cap and remove it.                    2

                                                                   1 Top of the fuel tank
                                                                   2 Approximately 50 mm (2 in) from top of the
                                                                     fuel tank
                                                          1                                 1
                                                                                                 2

                              1 Fuel filler cap
                            (6) Slowly add fuel to the fuel tank.
                              Fuel tank capacity:
                                70 L (18.5 US gal, 15.4 Imp.gal)
                                                                   1 Top of the fuel tank
                                                                   2 Approximately 50 mm (2 in) from top of the
                                                                     fuel tank
                                                                  (8) Wipe up any spilled fuel immediately with
                                                                     a dry cloth.
                                                                  (9) Securely install the fuel filler cap by tight-
                                                                     ening it until it clicks.
                                                                  (10) Push the rear of the hood down to se-
                                                                     curely lock it in place. Make sure that the

                            (7) Stop filling  when the  fuel level reaches
                                approximately 50 mm (2 in) from the top

                            65

| 65 66 67 68 69 70 71 72 73 74 75 |