Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 42 - LIT-18626-11-73
P. 42

    UF3J14E0.book  Page 37  Friday, June 23, 2017  9:47 AM

                            Watercraft operation

                            and the “N” (neutral) shift indicator will be dis-  To shift into forward:
                            played.                               (1) Release the RiDE lever.
                                                                  (2) Squeeze the throttle lever. The reverse
                                                                     gate  will rise completely, the engine
                                               1
                                                                     speed will increase, the watercraft will
                                                                     start moving forward, and the “F” (for-
                                                                     ward) shift indicator will be displayed.

                                                                          1

                              1 RiDE lever

                                                    1

                                                                   1 Throttle lever

                                                                                       1
                                                          2

                              1 Reverse gate
                              2 Neutral position                                              2

                                      1

                                                                   1 Reverse gate
                                                                   2 Forward position

                                                                           1

                              1 “N” (Neutral position)
                            TIP:
                            Although the neutral position helps keep the
                            watercraft from moving even when the en-
                            gine is running, some movement may occur.
                                                                   1 “F” (Forward position)

                            37

| 37 38 39 40 41 42 43 44 45 46 47 |