Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 47 - LIT-18626-11-73
P. 47

    UF3J14E0.book  Page 42  Friday, June 23, 2017  9:47 AM

                                                                      Watercraft operation

                            To deactivate the no-wake mode:       TIP:
                            Perform one of the following operations. The  The beeps and the blinking digital speedom-
                            beeper sounds two times quickly and the di-  eter display also indicate the activation of the
                            gital speedometer display  stops  blinking  no-wake mode. (See page 41 for information
                            when the no-wake mode is deactivated.  on the no-wake mode.)
                             Push the “NO-WAKE MODE” switch.     To activate the cruise assist:
                             Squeeze the throttle lever.         (1) Operate the throttle lever until the de-
                             Squeeze the RiDE lever.                sired engine speed is reached.
                            TIP:                                  (2) When the engine speed reaches the de-
                            The no-wake mode is also deactivated when  sired cruise assist  setting, push  the
                            the engine is stopped.                   “SET” switch. Once the beeper sounds
                            EJU37029                                 three times quickly and the digital speed-
                            Cruise assist
                                                                     ometer display starts blinking, the cruise
                            The cruise assist is a function for maintaining
                                                                     assist is activated. When the cruise as-
                            a desired engine speed within a fixed range
                                                                     sist is activated, slowly squeeze  the
                            while operating the watercraft.
                                                                     throttle lever to keep it squeezed further
                            TIP:                                     than the position at which the cruise as-
                             The cruise assist can only be set between  sist was set; releasing the throttle lever
                              engine speeds of approximately 3000    will deactivate the cruise assist.
                              r/min and approximately 7000 r/min.
                                                                  TIP:
                             The cruise assist cannot be activated in the
                                                                  The digital speedometer display blinks con-
                              Low  RPM  Mode. (See page  40 for Low
                                                                  tinually  while the cruise assist is activated.
                              RPM Mode activation procedures.)
                                                                  Make sure that the beeper has sounded and
                            Activating and deactivating the cruise as-
                                                                  the  digital speedometer display  is blinking
                            sist
                                                                  before squeezing the throttle lever to the full
                            Activation of  the  cruise assist will be con-
                                                                  throttle position. If the speedometer display is
                            firmed by the number of beeps when the
                                                                  not blinking, the cruise assist is not activated
                            “SET” switch,  cruise assist up switch,  or
                            cruise assist down switch is pushed, and by
                            the digital speedometer display of the multi-
                            function information center. (See page 44 for
                            information on the multifunction information
                            center.)
                                                        Digital
                             Number   Cruise assist opera-
                             of beeps       tion      speedome-
                                                       ter display
                                                        Starts
                                          Activated
                                                        blinking
                                                        Stops
                                         Deactivated
                                                        blinking
                                      Set engine speed in-  Continues
                                      creases or decreases  blinking

                                                                                                   42

| 42 43 44 45 46 47 48 49 50 51 52 |