Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 46 - LIT-18626-11-73
P. 46

    UF3J14E0.book  Page 41  Friday, June 23, 2017  9:47 AM

                            Watercraft operation

                            To deactivate the Low RPM Mode:       TIP:
                            Push the “L-Mode” (unlock) button on the re-  The beeps and the blinking digital speedom-
                            mote control transmitter for more than 4 sec-  eter display also indicate the activation of the
                            onds. Once the beeper sounds two times and  cruise assist. (See page 42 for information on
                            the “UNLOCK” indicator  light blinks  two  the cruise assist.)
                            times, then comes on, the “L-MODE” indica-  To activate the no-wake mode:
                            tor light goes off and the Low RPM Mode is  (1) Release the throttle lever and let the en-
                            deactivated. When the Low RPM Mode is de-  gine speed return to idle.
                            activated, the watercraft returns to the nor-  (2) Push and hold the “NO-WAKE MODE”
                            mal operation mode.                      switch.  Once  the beeper sounds three
                            EJU42484
                            No-wake mode                             times quickly and “8” (when kilometers
                            The no-wake mode is a function that main-  are selected) or “5” (when miles are se-
                            tains the engine speed at a fixed setting for  lected)  starts  blinking in the digital
                            operating the watercraft at low speeds. This  speedometer display, the no-wake
                            function can be used only for forward water-  mode is activated. Keep the throttle lever
                            craft operation or when the watercraft is in  in the fully closed (idle) position when the
                            neutral.                                 no-wake mode is activated.
                            TIP:                                  TIP:
                             The no-wake mode can only be activated  The digital speedometer display blinks con-
                              after 5 seconds have elapsed since starting  tinually while the no-wake mode is activated.
                              the engine.
                             If the no-wake mode is activated when the
                              watercraft is operating in neutral, the  re-                      1
                              verse gate will move to the forward posi-
                              tion.
                            Activating and deactivating the no-wake
                            mode
                            Activation of the no-wake mode will be con-
                            firmed by the number of beeps when the
                            “NO-WAKE MODE” switch is pushed, and by
                            the digital speedometer display of the multi-  1 “NO-WAKE MODE” switch
                            function information center. (See page 44 for
                            information on the multifunction information
                            center.)
                                                        Digital
                             Number  No-wake mode oper-
                             of beeps      ation      speedome-
                                                       ter display
                                                        Starts
                                          Activated
                                                        blinking
                                                        Stops
                                         Deactivated
                                                        blinking

                            41

| 41 42 43 44 45 46 47 48 49 50 51 |