Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 115 - LIT-18626-11-73
P. 115

    UF3J14E0.book  Page 110  Friday, June 23, 2017  9:47 AM

                                                                           Trouble recovery

                            (3) Remove the electrical box cover.     Install the spare fuse,  and then  tighten
                                                                     the screws.
                             1                              3
                                                                     1 23       4  5       6 7

                                                          2                                     8
                                                        2                                       9
                                                   3

                                                                                                8
                              1 Electrical box cover                        10  11    5
                              2 Lock                               1 Electronic throttle valve fuse
                              3 Projection                         2 Fuel pump fuse
                            (4) While pushing both sides of the fuse box  3 Main relay drive fuse
                                                                   4 Main fuse
                                cover inward, pull the cover toward the
                                                                   5 Spare fuse
                                bow and remove it.
                                                                   6 Fuse puller
                                                                   7 Battery fuse
                                      1                            8 Screw
                                                                   9 SCU fuse (BCU fuse)
                                                                  10 Bilge pump fuse
                                                                  11 Security system fuse
                                                                  (6) When  replacing a fuse other than the
                                                                     SCU fuse, remove the  fuse  using the
                                                                     fuse puller. Install a spare fuse of the
                                                                     proper amperage.  WARNING! Do not
                                                                     use fuses of a different amperage than
                              1 Fuse box cover
                                                                     recommended. Substitution with  a
                            (5) When replacing the SCU fuse, remove
                                                                     fuse that has an improper rating can
                                the screws, and then remove the fuse.
                                                                     cause extensive electrical  system
                                                                     damage and possible fire. [EWJ00803]

                                                                                                 110

| 110 111 112 113 114 115 116 117 118 119 120 |