Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 56 - LIT-18626-11-73
P. 56

    UF3J14E0.book  Page 51  Friday, June 23, 2017  9:47 AM

                            Instrument operation

                            DE/RESET” button for less than 1 second.  “AV MPH” since the measurement was start-
                            The display mode changes in the following  ed.
                            order.

                                                         1

                                                                  Tripmeter
                              1 “MODE/RESET” button
                                                                  This display shows the distance traveled in
                            Compass (FX Cruiser SVHO / FX Limited   kilometers “KM” or miles “MILES” since the
                            SVHO)                                 measurement was started.
                            This  display shows the  current direction of
                            the watercraft using the  8 major  compass
                            points.
                            TIP:
                            The accuracy of the compass varies depend-
                            ing  on the operating  conditions. Use this
                            function as a reference only.

                                                                  Fuel consumption per hour
                                                                  This display shows the current fuel consump-
                                                                  tion in liters per hour “L/HR” or gallons per
                                                                  hour “G/HR”.

                            Average speed
                            This display shows the average speed in kilo-
                            meters per hour “AV KMH” or miles per hour

                            51

| 51 52 53 54 55 56 57 58 59 60 61 |