Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 36 - LIT-18626-11-73
P. 36

    UF3J14E0.book  Page 31  Friday, June 23, 2017  9:47 AM

                            Control function operation

                            two conditions: (1) this device may not cause
                                                                                               “UN-
                            harmful interference, and (2) this device must  Number of   Yamaha Security  LOCK” in-
                            accept  any interference received, including  beeps  System mode  dicator
                                                                                               light
                            interference that may cause undesired oper-
                            ation.                                                 Lock       Goes off
                            ECJ00031                                              Unlock      Comes
                             NOTICE                                           (normal operation   on
                                                                                  mode)
                            Changes or modifications not  expressly
                                                                                  Unlock      Comes
                            approved by the party responsible for             (Low RPM Mode)    on
                            compliance could void the user’s authority
                            to operate the remote control transmitter.  TIP:
                                                                   The beeper sounds two times for the nor-
                            EJU31385
                            Yamaha Security System                 mal operation mode or three times for the
                            The  Yamaha  Security System functions to  Low RPM Mode. (See  page 40  for Low
                            help prevent unauthorized use or theft of the  RPM Mode activation procedures.)
                            watercraft. The lock and unlock modes of the   If the remote control transmitter is operated
                            security system can be selected by operating  while the multifunction information center
                            the remote control transmitter that is included  is in the standby state, the center will per-
                            with  this watercraft. The engine  cannot  be  form the initial operation, and then the set-
                            started if the lock mode of the security sys-  ting is selected.
                            tem is selected. The engine can only be start-  To select the lock mode:
                            ed if the unlock mode is selected. (See page  Push the lock button on the remote control
                            30 for information on the remote control  transmitter briefly. The beeper sounds once
                            transmitter.)                         and the “UNLOCK” indicator light  blinks
                                                                  once, then goes off. This indicates the lock
                            TIP:
                                                                  mode is selected.
                            The  Yamaha  Security System settings can
                            only be selected while the engine is stopped.  1
                            EJU36776                                                   2
                            Yamaha Security System settings
                            The Yamaha Security System settings will be
                            confirmed by the number of beeps when the
                            remote control transmitter is operated, and
                            by the “UNLOCK” indicator light of the multi-
                            function information center. (See page 44 for
                            information on the multifunction information
                            center.)
                                                                   1 Lock button
                                                                   2 “UNLOCK” indicator light
                                                                  To select the unlock mode:
                                                                  Push the “L-Mode” (unlock) button on the re-
                                                                  mote control transmitter briefly. The beeper
                                                                  sounds two  or  three times  and the “UN-

                            31

| 31 32 33 34 35 36 37 38 39 40 41 |