Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 84 - LIT-18626-11-73
P. 84

    UF3J14E0.book  Page 79  Friday, June 23, 2017  9:47 AM

                            Pre-operation checks

                            flood the engine compartment and cause  EJU40146
                                                                  Post-launch checks
                            the watercraft to submerge. [ECJ00363]
                                                                  Perform the post-launch checks in the pre-
                                                                  operation checklist while the watercraft is in
                                                                  the water and the engine is running.
                                                                  To perform the post-launch checks:
                                                           2      (1) Launch the watercraft. (See page 82 for
                                                           1         information on launching the watercraft.)
                                                                  (2) Perform the checks and make sure that
                                                                     there are no malfunctioning items or oth-
                                                                     er problems.
                                                                  EJU41811
                                                                  Cooling water pilot outlet check
                              1 Stern drain plug                  Make sure that water is discharged from the
                              2 O-ring
                                                                  port (left) cooling water pilot outlet while the
                            Securely install the stern drain plugs by tight-  engine is running. (See page 35 for informa-
                            ening them until they stop.           tion on the cooling water pilot outlets.)
                                                             1

                              1 Stern drain plug                  EJU32715
                                                                  Multifunction information center check
                            EJU41441
                            Hood check                            Make sure that the multifunction information
                            Push down on the rear of the hood and make  center operates properly. (See page 44 for in-
                            sure that it is securely closed.

                            79

| 79 80 81 82 83 84 85 86 87 88 89 |