Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 49 - LIT-18626-11-73
P. 49

    UF3J14E0.book  Page 44  Friday, June 23, 2017  9:47 AM

                                                                     Instrument operation

                            EJU42241                              segments and indicator lights come on. After
                                Multifunction information
                                                                  2 seconds, the  “WARNING” indicator light
                                          center                  and the warning indicators in the information
                            The multifunction information center displays  display go off, and then the center starts to
                            various watercraft information.       operate normally.
                                  1  2       3 4     5   6        TIP:
                                                                  The “UNLOCK” indicator  light will  go  off
                                                                  when the engine is started.
                                                                  Multifunction information center standby
                                                                  state
                                                                  If the multifunction information center does
                                                                  not receive any operation input within 25 sec-
                                                                  onds after the engine stops, the center will
                                                                  turn off and enter a standby state. When the
                                               7  8
                                                                  engine is started again, the displays return to
                              1 Information display
                                                                  their state before the center turned off, and
                              2 “UNLOCK” indicator light
                                                                  then the center starts to operate normally.
                              3 Analog speedometer/tachometer
                                                                  EJU42331
                              4 “WARNING” indicator light
                                                                  Analog speedometer/tachometer
                              5 “L-MODE” indicator light
                                                                  The  analog speedometer/tachometer has
                              6 Multifunction display
                                                                  both a speedometer function and a tachom-
                              7 “RPM” indicator light
                                                                  eter function. By switching the meter, it can
                              8 “SPEED” indicator light
                                                                  be  used  as either  a speedometer or a ta-
                                                                  chometer.
                                                                  TIP:
                                          1    2   3   4
                                                                  The analog tachometer is selected at  the
                                                                  Yamaha factory.

                              1 “SPEED/RPM” button
                              2 “VOLT/HOUR” button
                              3 “START/STOP” button
                              4 “MODE/RESET” button
                            Multifunction information center initial op-
                            eration                               Analog tachometer
                            When the multifunction information center is  The  analog  tachometer shows the engine
                            activated, the analog speedometer/tachome-  speed.
                            ter makes one sweep, and all of the display

                                                                                                   44

| 44 45 46 47 48 49 50 51 52 53 54 |