Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 40 - LIT-18626-11-73
P. 40

    UF3J14E0.book  Page 35  Friday, June 23, 2017  9:47 AM

                            Control function operation

                            (2) Make sure that the tilt lever returns to its  TIP:
                                original position and that the handlebars   It will take about 60 seconds for the water
                                are securely locked in place.      to reach the outlets after the engine is start-
                                                                   ed.
                                                                   Water  discharge may not be  constant
                                                                   when the engine is running at idling speed.
                                                                   If this occurs, apply a little throttle to make
                                                                   sure that water discharges properly.
                                                                  EJU40323
                                                                  Water separator
                                                                  The water separator prevents water from en-
                                                                  tering the fuel tank by collecting any water
                                                                  that has entered the fuel tank breather hose if
                                                                  the watercraft was capsized.
                            EJU41801
                            Cooling water pilot outlets           If water has collected in the water separator,
                            When the engine  is running, some of  the  drain it by loosening the drain screw.
                            cooling water that is circulated in the engine
                            is discharged from  the cooling  water pilot
                            outlets.                                                              1
                                                                                                  2

                                                                   1 Water separator
                               1                                   2 Drain screw
                                                                  To drain water from the water separator:
                              1 Cooling water pilot outlet (port [left] side)
                                                                  (1) Place a drain pan or dry cloth under the
                            There are cooling water pilot outlets on the  water separator.
                            port (left) and starboard (right) sides of the  (2) Gradually loosen the drain screw to drain
                            watercraft. To check for proper operation of  the water. Catch the draining water in the
                            the cooling system, make sure that water is  drain pan or soak it up with the dry cloth
                            being discharged from the port (left) pilot out-  so that it does not spill into the engine
                            let. If water is not being discharged from the  compartment. If any water spills into the
                            outlet, stop the engine and check the jet in-  watercraft, be sure to wipe it up with a
                            take for clogging. (See page 107 for informa-  dry cloth.
                            tion on the jet intake.)              (3) Securely tighten the drain screw until it
                                                                     stops.

                            35

| 35 36 37 38 39 40 41 42 43 44 45 |