Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 113 - LIT-18626-11-73
P. 113

    UF3J14E0.book  Page 108  Friday, June 23, 2017  9:47 AM

                                                                           Trouble recovery

                                ler, jet pump housing, and jet thrust noz-  (4) Raise the reverse gate to the forward po-
                                zle.                                 sition.
                                If debris is difficult to remove, consult a
                                Yamaha dealer.                                         1
                            EJU43472
                            Raising the reverse gate
                            If the RiDE system malfunctions and the re-
                            verse gate remains in the lowered position,
                            the watercraft will not be able to move for-                      2
                            ward.
                            After raising the reverse gate so that the wa-
                            tercraft can move  forward, immediately  re-
                            turn to shore and have a  Yamaha dealer  1 Reverse gate
                            service the watercraft.                2 Forward position
                            To raise the reverse gate:
                                                                  TIP:
                            (1) Stop the engine and remove the clip from
                                the engine shut-off switch.        While the shift rod is disconnected, the re-
                            (2) Enter the water and move to the rear of  verse gate will not move to the neutral po-
                                the watercraft.                    sition or reverse position even if the RiDE
                            (3) Slide the shift rod joint toward the bow,  lever is squeezed.
                                and then disconnect the shift rod joint   If the RiDE lever is squeezed while the shift
                                from the ball joint.               rod is disconnected, the watercraft will
                                                                   move forward.
                                                                  EJU34642
                                                                  Jumping the battery
                                                                  If the watercraft battery has run down, the en-
                                                                  gine can be started using a 12-volt booster
                                                                  battery and jumper cables.
                                                  1        2      EJU34664
                                                                  Connecting the jumper cables
                                                                  EWJ01251
                                                                      WARNING
                                                                  To avoid battery explosion  and serious
                              1 Shift rod joint                   damage to the electrical system:
                              2 Ball joint                         Do not reverse the polarity of the jumper
                                                                   cables when connecting to the batter-
                                                                   ies.
                                                                   Do not connect the negative (–) jumper
                                                                   cable to the negative (–) terminal of the
                                                                   watercraft battery.
                                                                   Do not touch the positive (+) jumper ca-
                                                                   ble to the negative (–) jumper cable.

                                                                                                 108

| 108 109 110 111 112 113 114 115 116 117 118 |